<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.30.0-'s-Hertogenbosch">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract></abstract>
  <contact>
    <name></name>
    <organization></organization>
    <position></position>
    <voice></voice>
    <fax></fax>
    <email></email>
    <role></role>
  </contact>
  <links/>
  <dates/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys nativeFormat="Wkt">
      <wkt>BOUNDCRS[SOURCECRS[PROJCRS["unknown",BASEGEOGCRS["unknown",DATUM["Unknown based on Bessel 1841 ellipsoid using towgs84=674.374,15.056,405.346,0,0,0,0",ELLIPSOID["Bessel 1841",6377397.155,299.1528128,LENGTHUNIT["metre",1,ID["EPSG",9001]]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8901]]],CONVERSION["unknown",METHOD["Hotine Oblique Mercator (variant B)",ID["EPSG",9815]],PARAMETER["Latitude of projection centre",46.9524055555556,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8811]],PARAMETER["Longitude of projection centre",7.43958333333333,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8812]],PARAMETER["Azimuth of initial line",90,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8813]],PARAMETER["Angle from Rectified to Skew Grid",90,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8814]],PARAMETER["Scale factor on initial line",1,SCALEUNIT["unity",1],ID["EPSG",8815]],PARAMETER["Easting at projection centre",2600000,LENGTHUNIT["metre",1],ID["EPSG",8816]],PARAMETER["Northing at projection centre",1200000,LENGTHUNIT["metre",1],ID["EPSG",8817]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1,ID["EPSG",9001]]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1,ID["EPSG",9001]]]]],TARGETCRS[GEOGCRS["WGS 84",DATUM["World Geodetic System 1984",ELLIPSOID["WGS 84",6378137,298.257223563,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],CS[ellipsoidal,2],AXIS["latitude",north,ORDER[1],ANGLEUNIT["degree",0.0174532925199433]],AXIS["longitude",east,ORDER[2],ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4326]]],ABRIDGEDTRANSFORMATION["Transformation from unknown to WGS84",METHOD["Position Vector transformation (geog2D domain)",ID["EPSG",9606]],PARAMETER["X-axis translation",674.374,ID["EPSG",8605]],PARAMETER["Y-axis translation",15.056,ID["EPSG",8606]],PARAMETER["Z-axis translation",405.346,ID["EPSG",8607]],PARAMETER["X-axis rotation",0,ID["EPSG",8608]],PARAMETER["Y-axis rotation",0,ID["EPSG",8609]],PARAMETER["Z-axis rotation",0,ID["EPSG",8610]],PARAMETER["Scale difference",1,ID["EPSG",8611]]]]</wkt>
      <proj4>+proj=somerc +lat_0=46.9524055555556 +lon_0=7.43958333333333 +k_0=1 +x_0=2600000 +y_0=1200000 +ellps=bessel +towgs84=674.374,15.056,405.346,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>47</srsid>
      <srid>2056</srid>
      <authid>EPSG:2056</authid>
      <description>CH1903+ / LV95</description>
      <projectionacronym>somerc</projectionacronym>
      <ellipsoidacronym>PARAMETER:6377397.15500000026077032:6356078.96281818859279156</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent>
    <spatial maxz="0" miny="0" dimensions="2" minz="0" maxx="0" maxy="0" crs="EPSG:2056" minx="0"/>
    <temporal>
      <period>
        <start></start>
        <end></end>
      </period>
    </temporal>
  </extent>
</qgis>
