<!DOCTYPE qgis PUBLIC 'http://mrcc.com/qgis.dtd' 'SYSTEM'>
<qgis version="3.22.13-Bia?owie?a">
  <identifier></identifier>
  <parentidentifier></parentidentifier>
  <language></language>
  <type>dataset</type>
  <title></title>
  <abstract>Potentiel de désimperméabilisation des sols - SDT pour PDcom - Terasol - 2024</abstract>
  <links/>
  <fees></fees>
  <encoding></encoding>
  <crs>
    <spatialrefsys>
      <wkt>PROJCRS["CH1903+ / LV95",BASEGEOGCRS["CH1903+",DATUM["CH1903+",ELLIPSOID["Bessel 1841",6377397.155,299.1528128,LENGTHUNIT["metre",1]]],PRIMEM["Greenwich",0,ANGLEUNIT["degree",0.0174532925199433]],ID["EPSG",4150]],CONVERSION["Swiss Oblique Mercator 1995",METHOD["Hotine Oblique Mercator (variant B)",ID["EPSG",9815]],PARAMETER["Latitude of projection centre",46.9524055555556,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8811]],PARAMETER["Longitude of projection centre",7.43958333333333,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8812]],PARAMETER["Azimuth of initial line",90,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8813]],PARAMETER["Angle from Rectified to Skew Grid",90,ANGLEUNIT["degree",0.0174532925199433],ID["EPSG",8814]],PARAMETER["Scale factor on initial line",1,SCALEUNIT["unity",1],ID["EPSG",8815]],PARAMETER["Easting at projection centre",2600000,LENGTHUNIT["metre",1],ID["EPSG",8816]],PARAMETER["Northing at projection centre",1200000,LENGTHUNIT["metre",1],ID["EPSG",8817]]],CS[Cartesian,2],AXIS["(E)",east,ORDER[1],LENGTHUNIT["metre",1]],AXIS["(N)",north,ORDER[2],LENGTHUNIT["metre",1]],USAGE[SCOPE["Cadastre, engineering survey, topographic mapping (large and medium scale)."],AREA["Liechtenstein; Switzerland."],BBOX[45.82,5.96,47.81,10.49]],ID["EPSG",2056]]</wkt>
      <proj4>+proj=somerc +lat_0=46.9524055555556 +lon_0=7.43958333333333 +k_0=1 +x_0=2600000 +y_0=1200000 +ellps=bessel +towgs84=674.374,15.056,405.346,0,0,0,0 +units=m +no_defs</proj4>
      <srsid>47</srsid>
      <srid>2056</srid>
      <authid>EPSG:2056</authid>
      <description>CH1903+ / LV95</description>
      <projectionacronym>somerc</projectionacronym>
      <ellipsoidacronym>EPSG:7004</ellipsoidacronym>
      <geographicflag>false</geographicflag>
    </spatialrefsys>
  </crs>
  <extent/>
</qgis>
